<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="160" y2="0" width="0" layer="20"/>
<wire x1="160" y1="0" x2="160" y2="100" width="0" layer="20"/>
<wire x1="160" y1="100" x2="0" y2="100" width="0" layer="20"/>
<wire x1="0" y1="100" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="dp_devices">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="DIL16">
<description>DIL-16</description>
</package>
</packages>
</library>
<library name="Atmel">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 14:02:49</description>
<packages>
<package name="DIP254P762X457-28">
</package>
</packages>
</library>
<library name="74ttl-din">
<description>&lt;b&gt;TTL Devices with DIN Symbols&lt;/b&gt;&lt;p&gt;
CadSoft and the author do not warrant that this library is free from error
or will meet your specific requirements.&lt;p&gt;
&lt;author&gt;Created by Holger Bettenbühl, hol.bet.@rhein-main.net&lt;/author&gt;</description>
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="TC38H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC33U-V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="LED5MMRGB">
</package>
<package name="TO92-EBC-OVAL">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
grid 5.08 mm</description>
</package>
</packages>
</library>
<library name="russian-nixies">
<description>&lt;b&gt;Russian IN series nixie tubes&lt;/b&gt;&lt;br&gt;&lt;br&gt;

Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Measurements taken from nixies in my collection
&lt;li&gt;http://www.tube-tester.com
&lt;/ul&gt;&lt;br&gt;
&lt;author&gt;Created by p.s.troost@student.tue.nl&lt;/author&gt;</description>
<packages>
<package name="IN-8">
<description>May be used with socket: &lt;b&gt;11-pin- Russian&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="DISCRETE">
<packages>
<package name="R-12,5">
</package>
<package name="C-5">
</package>
</packages>
</library>
<library name="BATTERY">
<description>&lt;b&gt;Lithium Batteries and NC Accus&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="NC-MM">
<description>&lt;b&gt;NC ACCU&lt;/b&gt; Sonnenschein&lt;p&gt;
Mini-Memo NC-MM&lt;p&gt;
2.4 to 4.8 R5</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="dp_devices" package="DIL16" value="IC_74141-DIP-16"/>
<element name="IC2" library="dp_devices" package="DIL16" value="IC_74141-DIP-16"/>
<element name="IC3" library="dp_devices" package="DIL16" value="IC_74141-DIP-16"/>
<element name="IC4" library="dp_devices" package="DIL16" value="IC_74141-DIP-16"/>
<element name="IC5" library="dp_devices" package="DIL16" value="IC_74141-DIP-16"/>
<element name="IC6" library="dp_devices" package="DIL16" value="IC_74141-DIP-16"/>
<element name="U1" library="Atmel" package="DIP254P762X457-28" value="ATMEGA328P-PU">
<attribute name="PACKAGE" value="PDIP-28"/>
<attribute name="OC_NEWARK" value="15R0268"/>
<attribute name="MPN" value="ATMEGA328P-PU"/>
<attribute name="SUPPLIER" value="Atmel"/>
<attribute name="OC_FARNELL" value="1715487"/>
</element>
<element name="V1" library="74ttl-din" package="DIL16" value="74595N"/>
<element name="V2" library="74ttl-din" package="DIL16" value="74595N"/>
<element name="V3" library="74ttl-din" package="DIL16" value="74595N"/>
<element name="IC7" library="adafruit" package="DIL08" value="DS1307"/>
<element name="Q1" library="adafruit" package="TC38H" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="Q2" library="adafruit" package="HC33U-V" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="N1" library="russian-nixies" package="IN-8" value="IN-8"/>
<element name="N2" library="russian-nixies" package="IN-8" value="IN-8"/>
<element name="N3" library="russian-nixies" package="IN-8" value="IN-8"/>
<element name="N4" library="russian-nixies" package="IN-8" value="IN-8"/>
<element name="N5" library="russian-nixies" package="IN-8" value="IN-8"/>
<element name="N6" library="russian-nixies" package="IN-8" value="IN-8"/>
<element name="R1" library="DISCRETE" package="R-12,5" value=""/>
<element name="R2" library="DISCRETE" package="R-12,5" value=""/>
<element name="R3" library="DISCRETE" package="R-12,5" value=""/>
<element name="R4" library="DISCRETE" package="R-12,5" value=""/>
<element name="R5" library="DISCRETE" package="R-12,5" value=""/>
<element name="R6" library="DISCRETE" package="R-12,5" value=""/>
<element name="R7" library="DISCRETE" package="R-12,5" value=""/>
<element name="R8" library="DISCRETE" package="R-12,5" value=""/>
<element name="R9" library="DISCRETE" package="R-12,5" value=""/>
<element name="R10" library="DISCRETE" package="R-12,5" value=""/>
<element name="R11" library="DISCRETE" package="R-12,5" value=""/>
<element name="R12" library="DISCRETE" package="R-12,5" value=""/>
<element name="LED1" library="adafruit" package="LED5MMRGB" value="RGBLED_CA-5MM"/>
<element name="LED2" library="adafruit" package="LED5MMRGB" value="RGBLED_CA-5MM"/>
<element name="LED3" library="adafruit" package="LED5MMRGB" value="RGBLED_CA-5MM"/>
<element name="LED4" library="adafruit" package="LED5MMRGB" value="RGBLED_CA-5MM"/>
<element name="LED5" library="adafruit" package="LED5MMRGB" value="RGBLED_CA-5MM"/>
<element name="LED6" library="adafruit" package="LED5MMRGB" value="RGBLED_CA-5MM"/>
<element name="T1" library="adafruit" package="TO92-EBC-OVAL" value="2N2222"/>
<element name="T2" library="adafruit" package="TO92-EBC-OVAL" value="2N2222"/>
<element name="T3" library="adafruit" package="TO92-EBC-OVAL" value="2N2222"/>
<element name="R13" library="DISCRETE" package="R-12,5" value=""/>
<element name="R14" library="DISCRETE" package="R-12,5" value=""/>
<element name="R15" library="DISCRETE" package="R-12,5" value=""/>
<element name="C1" library="DISCRETE" package="C-5" value=""/>
<element name="C2" library="DISCRETE" package="C-5" value=""/>
<element name="G1" library="BATTERY" package="NC-MM" value="NC-MM2V4"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="U1" pad="7"/>
<contactref element="IC7" pad="8"/>
</signal>
<signal name="AVCC">
<contactref element="U1" pad="20"/>
</signal>
<signal name="+UB">
<contactref element="V1" pad="16"/>
<contactref element="V2" pad="16"/>
<contactref element="V3" pad="16"/>
</signal>
<signal name="-UB">
<contactref element="V1" pad="8"/>
<contactref element="V2" pad="8"/>
<contactref element="V3" pad="8"/>
</signal>
<signal name="N$1">
<contactref element="V1" pad="15"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="6"/>
<contactref element="V1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="7"/>
<contactref element="V1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="V1" pad="3"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="IC2" pad="3"/>
<contactref element="V1" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="IC2" pad="6"/>
<contactref element="V1" pad="5"/>
</signal>
<signal name="N$7">
<contactref element="IC2" pad="7"/>
<contactref element="V1" pad="6"/>
</signal>
<signal name="N$8">
<contactref element="IC2" pad="4"/>
<contactref element="V1" pad="7"/>
</signal>
<signal name="N$9">
<contactref element="V2" pad="15"/>
<contactref element="IC3" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="IC3" pad="6"/>
<contactref element="V2" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="V2" pad="2"/>
<contactref element="IC3" pad="7"/>
</signal>
<signal name="N$12">
<contactref element="IC3" pad="4"/>
<contactref element="V2" pad="3"/>
</signal>
<signal name="N$13">
<contactref element="IC4" pad="3"/>
<contactref element="V2" pad="4"/>
</signal>
<signal name="N$14">
<contactref element="IC4" pad="6"/>
<contactref element="V2" pad="5"/>
</signal>
<signal name="N$15">
<contactref element="IC4" pad="7"/>
<contactref element="V2" pad="6"/>
</signal>
<signal name="N$16">
<contactref element="V2" pad="7"/>
<contactref element="IC4" pad="4"/>
</signal>
<signal name="N$17">
<contactref element="V3" pad="15"/>
<contactref element="IC5" pad="3"/>
</signal>
<signal name="N$18">
<contactref element="IC5" pad="6"/>
<contactref element="V3" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="V3" pad="2"/>
<contactref element="IC5" pad="7"/>
</signal>
<signal name="N$20">
<contactref element="IC5" pad="4"/>
<contactref element="V3" pad="3"/>
</signal>
<signal name="N$21">
<contactref element="IC6" pad="3"/>
<contactref element="V3" pad="4"/>
</signal>
<signal name="N$22">
<contactref element="IC6" pad="6"/>
<contactref element="V3" pad="5"/>
</signal>
<signal name="N$23">
<contactref element="IC6" pad="7"/>
<contactref element="V3" pad="6"/>
</signal>
<signal name="N$24">
<contactref element="V3" pad="7"/>
<contactref element="IC6" pad="4"/>
</signal>
<signal name="N$25">
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="N1" pad="A"/>
</signal>
<signal name="N$27">
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="N2" pad="A"/>
</signal>
<signal name="N$28">
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="N3" pad="A"/>
</signal>
<signal name="N$31">
<contactref element="R7" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="N4" pad="A"/>
</signal>
<signal name="N$33">
<contactref element="R9" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="N5" pad="A"/>
</signal>
<signal name="N$35">
<contactref element="R11" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="N6" pad="A"/>
</signal>
<signal name="N$26">
<contactref element="N1" pad="1"/>
<contactref element="IC1" pad="15"/>
</signal>
<signal name="N$30">
<contactref element="IC1" pad="8"/>
<contactref element="N1" pad="2"/>
</signal>
<signal name="N$32">
<contactref element="N1" pad="3"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="N$34">
<contactref element="IC1" pad="13"/>
<contactref element="N1" pad="4"/>
</signal>
<signal name="N$36">
<contactref element="N1" pad="5"/>
<contactref element="IC1" pad="14"/>
</signal>
<signal name="N$37">
<contactref element="IC1" pad="11"/>
<contactref element="N1" pad="6"/>
</signal>
<signal name="N$38">
<contactref element="N1" pad="7"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="N$39">
<contactref element="IC1" pad="1"/>
<contactref element="N1" pad="8"/>
</signal>
<signal name="N$40">
<contactref element="N1" pad="9"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$41">
<contactref element="IC1" pad="16"/>
<contactref element="N1" pad="0"/>
</signal>
<signal name="N$42">
<contactref element="N2" pad="1"/>
<contactref element="IC2" pad="15"/>
</signal>
<signal name="N$43">
<contactref element="IC2" pad="8"/>
<contactref element="N2" pad="2"/>
</signal>
<signal name="N$44">
<contactref element="N2" pad="3"/>
<contactref element="IC2" pad="9"/>
</signal>
<signal name="N$45">
<contactref element="IC2" pad="13"/>
<contactref element="N2" pad="4"/>
</signal>
<signal name="N$46">
<contactref element="N2" pad="5"/>
<contactref element="IC2" pad="14"/>
</signal>
<signal name="N$47">
<contactref element="IC2" pad="11"/>
<contactref element="N2" pad="6"/>
</signal>
<signal name="N$48">
<contactref element="N2" pad="7"/>
<contactref element="IC2" pad="10"/>
</signal>
<signal name="N$49">
<contactref element="IC2" pad="1"/>
<contactref element="N2" pad="8"/>
</signal>
<signal name="N$50">
<contactref element="N2" pad="9"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="N$51">
<contactref element="IC2" pad="16"/>
<contactref element="N2" pad="0"/>
</signal>
<signal name="N$52">
<contactref element="N3" pad="1"/>
<contactref element="IC3" pad="15"/>
</signal>
<signal name="N$53">
<contactref element="IC3" pad="8"/>
<contactref element="N3" pad="2"/>
</signal>
<signal name="N$54">
<contactref element="N3" pad="3"/>
<contactref element="IC3" pad="9"/>
</signal>
<signal name="N$55">
<contactref element="IC3" pad="13"/>
<contactref element="N3" pad="4"/>
</signal>
<signal name="N$56">
<contactref element="N3" pad="5"/>
<contactref element="IC3" pad="14"/>
</signal>
<signal name="N$57">
<contactref element="IC3" pad="11"/>
<contactref element="N3" pad="6"/>
</signal>
<signal name="N$58">
<contactref element="N3" pad="7"/>
<contactref element="IC3" pad="10"/>
</signal>
<signal name="N$59">
<contactref element="IC3" pad="1"/>
<contactref element="N3" pad="8"/>
</signal>
<signal name="N$60">
<contactref element="N3" pad="9"/>
<contactref element="IC3" pad="2"/>
</signal>
<signal name="N$61">
<contactref element="IC3" pad="16"/>
<contactref element="N3" pad="0"/>
</signal>
<signal name="N$62">
<contactref element="IC4" pad="15"/>
<contactref element="N4" pad="1"/>
</signal>
<signal name="N$63">
<contactref element="N4" pad="2"/>
<contactref element="IC4" pad="8"/>
</signal>
<signal name="N$64">
<contactref element="IC4" pad="9"/>
<contactref element="N4" pad="3"/>
</signal>
<signal name="N$65">
<contactref element="N4" pad="4"/>
<contactref element="IC4" pad="13"/>
</signal>
<signal name="N$66">
<contactref element="IC4" pad="14"/>
<contactref element="N4" pad="5"/>
</signal>
<signal name="N$67">
<contactref element="N4" pad="6"/>
<contactref element="IC4" pad="11"/>
</signal>
<signal name="N$68">
<contactref element="IC4" pad="10"/>
<contactref element="N4" pad="7"/>
</signal>
<signal name="N$69">
<contactref element="N4" pad="8"/>
<contactref element="IC4" pad="1"/>
</signal>
<signal name="N$70">
<contactref element="IC4" pad="2"/>
<contactref element="N4" pad="9"/>
</signal>
<signal name="N$71">
<contactref element="N4" pad="0"/>
<contactref element="IC4" pad="16"/>
</signal>
<signal name="N$72">
<contactref element="N5" pad="1"/>
<contactref element="IC5" pad="15"/>
</signal>
<signal name="N$73">
<contactref element="N5" pad="2"/>
<contactref element="IC5" pad="8"/>
</signal>
<signal name="N$74">
<contactref element="IC5" pad="9"/>
<contactref element="N5" pad="3"/>
</signal>
<signal name="N$75">
<contactref element="N5" pad="4"/>
<contactref element="IC5" pad="13"/>
</signal>
<signal name="N$76">
<contactref element="IC5" pad="14"/>
<contactref element="N5" pad="5"/>
</signal>
<signal name="N$77">
<contactref element="N5" pad="6"/>
<contactref element="IC5" pad="11"/>
</signal>
<signal name="N$78">
<contactref element="IC5" pad="10"/>
<contactref element="N5" pad="7"/>
</signal>
<signal name="N$79">
<contactref element="N5" pad="8"/>
<contactref element="IC5" pad="1"/>
</signal>
<signal name="N$80">
<contactref element="IC5" pad="2"/>
<contactref element="N5" pad="9"/>
</signal>
<signal name="N$81">
<contactref element="N5" pad="0"/>
<contactref element="IC5" pad="16"/>
</signal>
<signal name="N$82">
<contactref element="N6" pad="1"/>
<contactref element="IC6" pad="15"/>
</signal>
<signal name="N$83">
<contactref element="IC6" pad="8"/>
<contactref element="N6" pad="2"/>
</signal>
<signal name="N$84">
<contactref element="N6" pad="3"/>
<contactref element="IC6" pad="9"/>
</signal>
<signal name="N$85">
<contactref element="IC6" pad="13"/>
<contactref element="N6" pad="4"/>
</signal>
<signal name="N$86">
<contactref element="N6" pad="5"/>
<contactref element="IC6" pad="14"/>
</signal>
<signal name="N$87">
<contactref element="IC6" pad="11"/>
<contactref element="N6" pad="6"/>
</signal>
<signal name="N$88">
<contactref element="N6" pad="7"/>
<contactref element="IC6" pad="10"/>
</signal>
<signal name="N$89">
<contactref element="IC6" pad="1"/>
<contactref element="N6" pad="8"/>
</signal>
<signal name="N$90">
<contactref element="N6" pad="9"/>
<contactref element="IC6" pad="2"/>
</signal>
<signal name="N$91">
<contactref element="N6" pad="0"/>
<contactref element="IC6" pad="16"/>
</signal>
<signal name="N$92">
<contactref element="LED1" pad="1"/>
<contactref element="LED6" pad="1"/>
<contactref element="LED2" pad="1"/>
<contactref element="LED3" pad="1"/>
<contactref element="LED4" pad="1"/>
<contactref element="LED5" pad="1"/>
<contactref element="T1" pad="C"/>
</signal>
<signal name="N$93">
<contactref element="LED1" pad="3"/>
<contactref element="LED6" pad="3"/>
<contactref element="LED2" pad="3"/>
<contactref element="LED3" pad="3"/>
<contactref element="LED4" pad="3"/>
<contactref element="LED5" pad="3"/>
<contactref element="T2" pad="C"/>
</signal>
<signal name="N$94">
<contactref element="LED1" pad="4"/>
<contactref element="LED6" pad="4"/>
<contactref element="LED2" pad="4"/>
<contactref element="LED3" pad="4"/>
<contactref element="LED4" pad="4"/>
<contactref element="LED5" pad="4"/>
<contactref element="T3" pad="C"/>
</signal>
<signal name="N$95">
<contactref element="LED1" pad="2"/>
<contactref element="LED6" pad="2"/>
<contactref element="LED2" pad="2"/>
<contactref element="LED3" pad="2"/>
<contactref element="LED4" pad="2"/>
<contactref element="LED5" pad="2"/>
</signal>
<signal name="GND">
<contactref element="T1" pad="E"/>
<contactref element="T3" pad="E"/>
<contactref element="T2" pad="E"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="IC7" pad="4"/>
<contactref element="G1" pad="-"/>
</signal>
<signal name="N$96">
<contactref element="R13" pad="1"/>
<contactref element="T1" pad="B"/>
</signal>
<signal name="N$97">
<contactref element="T2" pad="B"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$98">
<contactref element="R15" pad="1"/>
<contactref element="T3" pad="B"/>
</signal>
<signal name="N$99">
<contactref element="Q1" pad="2"/>
<contactref element="IC7" pad="1"/>
</signal>
<signal name="N$100">
<contactref element="Q1" pad="1"/>
<contactref element="IC7" pad="2"/>
</signal>
<signal name="N$101">
<contactref element="Q2" pad="1"/>
<contactref element="U1" pad="9"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$102">
<contactref element="Q2" pad="2"/>
<contactref element="U1" pad="10"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$103">
<contactref element="U1" pad="28"/>
<contactref element="IC7" pad="6"/>
</signal>
<signal name="N$104">
<contactref element="U1" pad="27"/>
<contactref element="IC7" pad="5"/>
</signal>
<signal name="N$105">
<contactref element="IC7" pad="3"/>
<contactref element="G1" pad="+"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
